eCos Reference Manual
Prev |  | Next

# Chapter 39. Networking Stack Features

Since this networking package is based on BSD code, it is very complete and robust. The eCos implementation includes support for the following protocols:

- IPv4

- UDP

- TCP

- ICMP

- raw packet interface

- Multi-cast addressing

- IPv6 (including UDP, ICP, ICMP)

These additional features are also present in the package, but are not supported:

- Berkeley Packet Filter

- Uni-cast support

- Multi-cast routing

Prev | Home | Next
FreeBSD TCP/IP Stack port for eCos | Up | Freebsd TCP/IP stack port