eCos User Guide
Prev | Appendix A. Target Setup | Next

# VRC4375 Hardware Setup

For information about setting up the VRC4375 to run with RedBoot, consult the RedBoot User"s Guide. If using serial debugging, the serial line runs at 38400 baud 8-N-1 and should be connected to the debug host using the cable supplied with the board.

Prev | Home | Next
VR4300 Hardware Setup | Up | Atlas/Malta Hardware Setup