eCos User Guide
Prev | Appendix A. Target Setup | Next

# NEC CEB-V850/SB1 Hardware Setup

The instructions for setting up the CEB-V850/SB1 are virtually identical to those of the CEB-V850/SA1 above. The only significant differences are that pre-built loaders are available at loaders/v850-ceb_v850/v850sb1 within the eCos installation. Binaries supporting boards with both 16MHz and 8MHz clock speeds are supplied. Also when building applications, or rebuilding the stubs for a V850/SB1 target, then the V850 CPU variant must be changed in the CEB-V850 HAL to the SB1.

Prev | Home | Next
NEC CEB-V850/SA1 Hardware Setup | Up | i386 PC Hardware Setup