eCos Reference Manual
Prev | Chapter 32. µITRON API | Next

# Task-Dependent Synchronization Functions

These functions are fully supported in this release:

    ER sus_tsk(
        ID tskid )

    ER rsm_tsk(
        ID tskid )

    ER frsm_tsk(
        ID tskid )

    ER slp_tsk( void )

    ER tslp_tsk(
        TMO tmout )

    ER wup_tsk(
        ID tskid )

    ER can_wup(
        INT *p_wupcnt,    ID tskid )

## Error checking

The following conditions are only checked for, and only return errors if CYGSEM_UITRON_BAD_PARAMS_RETURN_ERRORS is enabled (see the configuration option “Return Error Codes for Bad Params”):

- invalid tskid; less than 1 or greater than CYGNUM_UITRON_TASKS returns E_ID

- `wup_tsk()` , `sus_tsk()` , `rsm_tsk()` , `frsm_tsk()` on the calling task returns E_OBJ

- dispatching is enabled in `tslp_tsk()` and `slp_tsk()` , or E_CTX

- tmout must be positive, otherwise E_PAR

- return value pointer in `can_wup()` is a valid pointer, or E_PAR

The following conditions are checked for, and can return error codes, regardless of the setting of CYGSEM_UITRON_BAD_PARAMS_RETURN_ERRORS:

- When create and delete functions `cre_tsk()` and `del_tsk()` are supported, all calls which use a valid task ID number check that the task exists; if not, E_NOEXS is returned

- `sus_tsk()` : the task must not be dormant, else E_OBJ

- `frsm/rsm_tsk()` : the task must be suspended, else E_OBJ

- `tslp/slp_tsk()` : return codes E_TMOUT, E_RLWAI and E_DLT are returned depending on the reason for terminating the sleep

- `wup_tsk()` and `can_wup()` : the task must not be dormant, or E_OBJ is returned

Prev | Home | Next
Task Management Functions | Up | Synchronization and Communication Functions