eCos User Guide
Prev |  | Next

# Appendix A. Target Setup

The following sections detail the setup of many of the targets supported by eCos.

Caution
This information is presented here only temporarily. It is intended that there will be separate documents detailing this information for each target in future releases. Consequently not much effort has been put into bringing the following documentation up to date -- much of it is obsolete, bogus or just plain wrong.

# MN10300 stdeval1 Hardware Setup

The eCos Developer’s Kit package comes with a pair of EPROMs which provide GDB support for the Matsushita MN10300 (AM31) series evaluation board using CygMon, the Cygnus ROM monitor. Images of these EPROMs are also provided at `BASE_DIR/loaders/mn10300-stdeval1/cygmon.bin`. The LSB EPROM (LROM) is installed to socket IC8 on the board and the MSB EPROM (UROM) is installed to socket IC9. Attention should be paid to the correct orientation of these EPROMs during installation.

The CygMon stubs allows communication with GDB by way of the serial port at connector CN2. The communication parameters are fixed at 38400 baud, 8 data bits, no parity bit, and 1 stop bit (8-N-1). No flow control is employed. Connection to the host computer should be made using a standard RS232C serial cable (not a null modem cable). A gender changer may also be required.

Prev | Home | Next
Appendixes | Up | MN10300 Architectural Simulator Setup