eCosPro® Reference Manual
Prev |  | Next

# Chapter 6. NAND Library Overview

# Description

This is a library which allows NAND flash devices to be accessed by the eCos kernel and applications. It is analogous to the eCos FLASH library, but for NAND devices. It exists as a separate library because of the fundamental differences between the two types of flash memory.

This library provides the following functionality:

- Interrogation to confirm that the expected device is present

- Reading from and writing to flash pages

- Erasing flash blocks

- The ability to divide a single device into multiple partitions, like those of a hard drive

- Creation and maintenance of a Bad Block Table

- Use of an Error Correcting Code to detect and correct single-bit errors, and to detect multiple-bit errors

- Packing of the ECC and application out-of-band data into the spare area on the device

> Note: The spare area, ECC and bad block table have been deliberately created with the intention of compatibility with current versions of the Linux MTD layer. For example, this would allow a single NAND device to be accessed by RedBoot to load a Linux kernel, which could then go on to use another partition as its root filesystem.

> Tip: This library is also used as glue to allow appropriate filesystems to use NAND devices. This allows more useful higher-level access by applications and RedBoot via the File I/O and POSIX interfaces. In other words, your application may not need to invoke this library directly, though of course you may still have to write a driver for your chip and/or board.

## Structure of the library

This library has two principal interfaces: one for applications to call into it, and another to call out to the chip-specific drivers. (The chip drivers themselves then require support from the relevant platform HAL to allow them to access the physical chip in an appropriate manner for the board - such as the memory-mapped I/O range to use.)

The following diagram illustrates the calls from two applications all the way to an underlying NAND device. Application 1 uses the NAND library directly, whereas application 2 is using a filesystem and the eCos File I/O layer.

## Device support

Before this library can be used on a given board, an appropriate device driver must be created. Each driver is for a particular NAND part or family of parts; the HAL for each board then instantiates the relevant driver(s) appropriately with board-specific glue such as the memory-mapped I/O range to use. Full details on creating a driver are presented in Chapter 8.

There is also a Synthetic Target NAND Flash Device for testing purposes, which is present on the synth target.

Prev | Home | Next
The eCos NAND Flash Library | Up | Danger, Will Robinson! Danger!