eCos Reference Manual
Prev | Chapter 47. CHAT Scripts | Next

# Sending EOT

The special reply string of EOT indicates that the chat program should send an EOT character to the remote. This is normally the End-of-file character sequence. A return character is not sent following the EOT. The EOT sequence may be embedded into the send string using the sequence "\x04" (i.e. a Control-D character).

Prev | Home | Next
TIMEOUT | Up | Escape Sequences