eCos User Guide
Prev | Chapter 11. Configuring and Building eCos from Source | Next

# Configuration Tool on Windows and Linux Quick Start

This section described the GUI based configuration tool. This tool is probably more suited to users who prefer GUI's. The next section describes a CLI based tool which Unix users may prefer.

Note that the use of the Configuration Tool is described in detail in Part IV in eCos User Guide.

The Configuration Tool (see Figure 11-1) has five main elements: the configuration window, the conflicts window, the properties window, the short description window, and the output window.

Figure 11-1. Configuration Tool

Start by opening the templates window via Build->Templates. Select the desired target (see Figure 11-2).

Figure 11-2. Template selection

Make sure that the configuration is correct for the target in terms of endianness, CPU model, Startup type, etc. (see Figure 11-3).

Figure 11-3. Configuring for the target

Next, select the Build->Library menu item to start building eCos (see Figure 11-4). The application will configure the sources, prepare a build tree, and build the `libtarget.a` library, which contains the eCos kernel and other packages.

Figure 11-4. Selecting the Build Library menu item

The Save As dialog box will appear, asking you to specify a directory in which to place your save file. You can use the default, but it is a good idea to make a subdirectory, called `ecos-work` for example.

Figure 11-5. Save file dialog

The first time you build an eCos library for a specific architecture, the Configuration Tool may prompt you for the location of the appropriate build tools (including make and TARGET-gcc) using a Build Tools dialog box (as shown in Figure 11-6). You can select a location from the drop down list, browse to the directory using the Browse button, or type in the location of the build tools manually.

Figure 11-6. Build tools dialog

The Configuration Tool may also prompt you for the location of the user tools (such as cat and ls) using a User Tools dialog box (as shown in Figure 11-7). As with the Build Tools dialog, you can select a location from the drop down list, browse to the directory using the Browse button, or type in the location of the user tools manually. Note that on Linux, this will often be unnecessary as the tools will already be on your PATH.

Figure 11-7. User tools dialog

When the tool locations have been entered, the Configuration Tool will configure the sources, prepare a build tree, and build the `libtarget.a` library, which contains the eCos kernel and other packages.

The output from the configuration process and the building of `libtarget.a` will be shown in the output window.

Once the build process has finished you will have a kernel with other packages in `libtarget.a`. You should now build the eCos tests for your particular configuration.

You can do this by selecting Build -> Tests. Notice that you could have selected Tests instead of Library in the earlier step and it would have built both the library and the tests, but this would increase the build time substantially, and if you do not need to build the tests it is unnecessary.

Figure 11-8. Selecting the Build Tests menu item

Chapter 12 will guide you through running one of the test cases you just built on the selected target, using GDB.

Prev | Home | Next
Configuring and Building eCos from Source | Up | Ecosconfig on Windows and Linux Quick Start