eCos Reference Manual
Prev | Chapter 55. The SNTP Client | Next

# What it does

The SNTP client listens for NTP IPv4 broadcasts from any NTP servers, or IPv6 multicasts using the address fe0x:0X::101, where X can be 2 (Link Local), 5 (Site-Local) or 0xe (Global). Such packets contain a timestamp indicating the current time. The packet also contains information about where the server is in the hierarchy of time servers. A server at the root of the time server tree normally has an atomic clock. Such a server is said to be at stratum 0. A time server which is synchronised to a stratum 0 server is said to be at stratum 1 etc. The client will accept any NTP packets from servers using version 3 or 4 of the protocol. When receiving packets from multiple servers, it will use the packets from the server with the lowest stratum. However, if there are no packets from this server for 10 minutes and another server is sending packets, the client will change servers.

If SNTP unicast mode is enabled via the CYGPKG_NET_SNTP_UNICAST option, the SNTP client can additionally be configured with a list of specific NTP servers to query. The general algorithm is as follows: if the system clock has not yet been set via an NTP time update, then the client will send out NTP requests every 30 seconds to all configured NTP servers. Once an NTP time update has been received, the client will send out additional NTP requests every 30 minutes in order to update the system clock. These requests are resent every 30 seconds until a response is received.

The system clock in eCos is accurate to 1 second. The SNTP client will change the system clock when the time difference with the received timestamp is greater than 2 seconds. The change is made as a step.

Prev | Home | Next
The SNTP Client | Up | Configuring the unicast list of NTP servers