eCosPro® Reference Manual
Prev | Chapter 5. Raw API | Next

# TCP connection setup

The functions used for setting up connections are similar to those of the sequential API and of the BSD socket API. A new TCP connection identifier (i.e., a protocol control block - PCB) is created with the `tcp_new()` function. This PCB can then be either set to listen for new incoming connections or be explicitly connected to another host.

Prev | Home | Next
tcp_arg() | Up | tcp_new()