eCos Reference Manual
Prev | Chapter 32. µITRON API | Next

# System Management Functions

These functions are fully supported in this release:

    ER get_ver(
        T_VER *pk_ver )

    ER ref_sys(
        T_RSYS *pk_rsys )

    ER ref_cfg(
        T_RCFG *pk_rcfg )

Note that the information returned by each of these calls may be configured to match the user's own versioning system, and the values supplied by the default configuration may be inappropriate.

These functions are not supported in this release:

    ER def_svc(
        FN s_fncd,
        T_DSVC *pk_dsvc )

    ER def_exc(
        UINT exckind,
        T_DEXC *pk_dexc )

## Error checking

The following conditions are only checked for, and only return errors if CYGSEM_UITRON_BAD_PARAMS_RETURN_ERRORS is enabled:

- return value pointer in all calls is a valid pointer, or E_PAR

Prev | Home | Next
Time Management Functions | Up | Network Support Functions