RedBoot User's Guide
Prev | Chapter 2. RedBoot Commands and Examples | Next

# Filesystem Interface

If the platform has access to secondary storage, then RedBoot may be able to access a filesystem stored on this device. RedBoot can access FAT filesystems stored on IDE disks or CompactFlash devices and can use JFFS2 filesystems stored in FLASH memory. The fs command is used to manipulate files on filesystems. Applications may be loaded into memory using the file mode of the load command.

Prev | Home | Next
fis write | Up | fs info